{"text_format":"3","workbook":"xlsx","n_sheets":4,"sheets":["汇总表","四楼","五楼","六楼"],"not_rendered":{"images":43,"defined_names":4},"read":"whole","date_system":"1900"}

{"sheet":"汇总表","index":0,"n_rows":6,"n_cols":3,"rows_kept":6,"merged":[[0,0,0,2],[5,0,5,1]]}
["汇创谷（盐城）科技企业孵化器办公家具采购项目 报价汇总表"]
["序号","楼层","总计价格（含税）"]
[1,"四楼"]
[2,"五楼"]
[3,"六楼"]
["合计"]

{"sheet":"四楼","index":1,"n_rows":56,"n_cols":11,"rows_kept":56,"merged":[[0,0,0,10],[2,0,2,10],[7,0,7,10],[12,0,12,10],[16,0,16,10],[19,0,19,10],[22,0,22,10],[25,0,25,10],[28,0,28,10],[31,0,31,10],[36,0,36,10],[44,0,44,10],[47,0,47,10],[50,0,50,10],[53,0,53,10],[55,0,55,9]]}
["汇创谷（盐城）科技企业孵化器办公家具采购项目（4楼） 报价清单"]
["序号","项目名称","图片","名称","颜色","材质说明","规格","单位","数量","单价","总价"]
["办公室（24平）"]
[1,"办公桌",{"$f":"_xlfn.DISPIMG(\"ID_E7C8D9E79B8C4C4384666A85E8FD048D\",1)","v":"=DISPIMG(\"ID_E7C8D9E79B8C4C4384666A85E8FD048D\",1)"},null,null,"1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。","1600*800*750","张",1]
[2,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_12AC6C0730724A9CA7144D411831E69C\",1)","v":"=DISPIMG(\"ID_12AC6C0730724A9CA7144D411831E69C\",1)"},null,null,"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；钢脚管壁2.0\"","椅宽640，椅高1200","张",1]
[3,"三人位",{"$f":"_xlfn.DISPIMG(\"ID_73A5BB03CE43475192FEF2E779AAE704\",1)","v":"=DISPIMG(\"ID_73A5BB03CE43475192FEF2E779AAE704\",1)"},null,null,"采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","1800*780*850","组",1]
[4,"茶几",{"$f":"_xlfn.DISPIMG(\"ID_1602EF315EAF4CC9B65DA1C0F9F6B15C\",1)","v":"=DISPIMG(\"ID_1602EF315EAF4CC9B65DA1C0F9F6B15C\",1)"},"办公桌","1200*600","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1200*600*400","组",1]
["办公室（26平）"]
[5,"办公桌",{"$f":"_xlfn.DISPIMG(\"ID_A9223FE190414E81A6A8DE4ED3840241\",1)","v":"=DISPIMG(\"ID_A9223FE190414E81A6A8DE4ED3840241\",1)"},null,"图片色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1600*800*750","张",1]
[6,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_340EEDC02EDF43E18E60B14AFE5F4707\",1)","v":"=DISPIMG(\"ID_340EEDC02EDF43E18E60B14AFE5F4707\",1)"},null,"图片色","1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；钢脚管壁2.0\"","椅宽640，椅高1200","张",1]
[7,"沙发",{"$f":"_xlfn.DISPIMG(\"ID_B7AC510567BD4BF19FD43A6AF4D487C0\",1)","v":"=DISPIMG(\"ID_B7AC510567BD4BF19FD43A6AF4D487C0\",1)"},null,"可定色","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","1800*780*850","张",1]
[8,"茶几",{"$f":"_xlfn.DISPIMG(\"ID_B6343B37C5E24C7DB4217238EA614702\",1)","v":"=DISPIMG(\"ID_B6343B37C5E24C7DB4217238EA614702\",1)"},null,"白色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1200*600*400","张",1]
["公共办公(140平)"]
[9,"6人位",{"$f":"_xlfn.DISPIMG(\"ID_72D2CBC327E64B3683FAE13517133107\",1)","v":"=DISPIMG(\"ID_72D2CBC327E64B3683FAE13517133107\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；      \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","3600*1200*750","张",4]
[10,"员工椅",{"$f":"_xlfn.DISPIMG(\"ID_2DF132A9B3224F5D93985C21727DCB45\",1)","v":"=DISPIMG(\"ID_2DF132A9B3224F5D93985C21727DCB45\",1)"},"牌桌椅子","灰色","1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽490，椅高1060","张",24]
[11,"低柜",{"$f":"_xlfn.DISPIMG(\"ID_2549137D035444E18AE4A40BB7ECA3CC\",1)","v":"=DISPIMG(\"ID_2549137D035444E18AE4A40BB7ECA3CC\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","3600*400*800","张",1]
["办公室"]
[12,"办公桌",{"$f":"_xlfn.DISPIMG(\"ID_E7F9B1035A9D48C78AFFA48797C86EEC\",1)","v":"=DISPIMG(\"ID_E7F9B1035A9D48C78AFFA48797C86EEC\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1600*800*750","张",1]
[13,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_D8CEC65BF12347C3B06E92D55B04488C\",1)","v":"=DISPIMG(\"ID_D8CEC65BF12347C3B06E92D55B04488C\",1)"},null,"可定色","1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽640，椅高1200","张",1]
["会议室"]
[14,"会议桌",{"$f":"_xlfn.DISPIMG(\"ID_6CC87A6C387A419FB4044323D5CE46D1\",1)","v":"=DISPIMG(\"ID_6CC87A6C387A419FB4044323D5CE46D1\",1)"},null,"白色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","3200*1400*750","张",1]
[15,"会议椅",{"$f":"_xlfn.DISPIMG(\"ID_1EDDF29948EA4A56AFB49AB18B2FAC2A\",1)","v":"=DISPIMG(\"ID_1EDDF29948EA4A56AFB49AB18B2FAC2A\",1)"},null,"白框橘","1、面料:选优质PU,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0","椅宽590，椅高900","张",8]
["办公室"]
[16,"办公桌",{"$f":"_xlfn.DISPIMG(\"ID_D25DBC3F057040C796B42EAFAC73233B\",1)","v":"=DISPIMG(\"ID_D25DBC3F057040C796B42EAFAC73233B\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1600*800*750","张",1]
[17,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_1986491C20E1422A9F46E317F7A7A940\",1)","v":"=DISPIMG(\"ID_1986491C20E1422A9F46E317F7A7A940\",1)"},null,null,"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽640，椅高1200","张",1]
["公共办公(175平)"]
[18,"十人位",{"$f":"_xlfn.DISPIMG(\"ID_52ACE1C22860492C8A47FA1E89919456\",1)","v":"=DISPIMG(\"ID_52ACE1C22860492C8A47FA1E89919456\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","6000*1200*750 ","组",2]
[19,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_F695620B63BC400C80132FDAFD28C885\",1)","v":"=DISPIMG(\"ID_F695620B63BC400C80132FDAFD28C885\",1)"},null,null,"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽490，椅高1060","张",20]
["休闲区"]
[20,"休闲沙发",{"$f":"_xlfn.DISPIMG(\"ID_00B8C1678B4E484C9045EC3FE282DA1B\",1)","v":"=DISPIMG(\"ID_00B8C1678B4E484C9045EC3FE282DA1B\",1)"},null,"胡桃色","采用优质布面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","2000*600*850","组",1]
[21,"茶几",{"$f":"_xlfn.DISPIMG(\"ID_076A5DE159BF408FBC0FEC4BCFC38C6B\",1)","v":"=DISPIMG(\"ID_076A5DE159BF408FBC0FEC4BCFC38C6B\",1)"},null,"灰白","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1200*600*400","组",1]
["办公区"]
[22,"办公桌",{"$f":"_xlfn.DISPIMG(\"ID_001E0BEC4CCC4A5D869710A6913FF938\",1)","v":"=DISPIMG(\"ID_001E0BEC4CCC4A5D869710A6913FF938\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1600*800*750","组",1]
[23,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_3C38E9ACAF1C44FAB59208CBCB60C375\",1)","v":"=DISPIMG(\"ID_3C38E9ACAF1C44FAB59208CBCB60C375\",1)"},null,"白橘","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽640，椅高1200","组",1]
[24,"沙发",{"$f":"_xlfn.DISPIMG(\"ID_3EBF93CCDC974212BFBBB315AAE05D04\",1)","v":"=DISPIMG(\"ID_3EBF93CCDC974212BFBBB315AAE05D04\",1)"},null,"可定色","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","1800*780*850","组",1]
[25,"茶几",{"$f":"_xlfn.DISPIMG(\"ID_BA09451684A54B45967BE1886E0E26BB\",1)","v":"=DISPIMG(\"ID_BA09451684A54B45967BE1886E0E26BB\",1)"},null,"白色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1200*600*400","张",1]
["办公室"]
[26,"办公桌",{"$f":"_xlfn.DISPIMG(\"ID_10FFBBA831574F2E9F3DBEAC2430277C\",1)","v":"=DISPIMG(\"ID_10FFBBA831574F2E9F3DBEAC2430277C\",1)"},null,"灰","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1600*800*750","张",1]
[27,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_572AC83351464CE1A6E2226E2AAD1E1F\",1)","v":"=DISPIMG(\"ID_572AC83351464CE1A6E2226E2AAD1E1F\",1)"},null,"白橘","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽640，椅高1200","张",1]
[28,"沙发",{"$f":"_xlfn.DISPIMG(\"ID_6ED4158B98A544F18607C1B18D9CEFF7\",1)","v":"=DISPIMG(\"ID_6ED4158B98A544F18607C1B18D9CEFF7\",1)"},null,"可定色","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","1800*780*850","张",1]
[29,"茶几",{"$f":"_xlfn.DISPIMG(\"ID_C0DD7CCD2EC14E51A863CB653F93247D\",1)","v":"=DISPIMG(\"ID_C0DD7CCD2EC14E51A863CB653F93247D\",1)"},null,"白","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1200*600*400","张",1]
[null,null,"办公区56平"]
[30,"六人位",{"$f":"_xlfn.DISPIMG(\"ID_C5BC302EE4FE48DE8A6B5143D807BB9B\",1)","v":"=DISPIMG(\"ID_C5BC302EE4FE48DE8A6B5143D807BB9B\",1)"},null,null,"1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","3600*1200*750","组",1]
[31,"员工椅",{"$f":"_xlfn.DISPIMG(\"ID_B5D6B95994284BD2A5BEAC695F8116B2\",1)","v":"=DISPIMG(\"ID_B5D6B95994284BD2A5BEAC695F8116B2\",1)"},null,"常规","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽490，椅高1060","张",6]
["办公室"]
[32,"办公桌",{"$f":"_xlfn.DISPIMG(\"ID_DD8BEC2ACCE649FDBE05B467CD19DB5B\",1)","v":"=DISPIMG(\"ID_DD8BEC2ACCE649FDBE05B467CD19DB5B\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1600*800*750","张",2]
[33,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_1943AF0C4F92412F86B3E13D16B1B409\",1)","v":"=DISPIMG(\"ID_1943AF0C4F92412F86B3E13D16B1B409\",1)"},null,"常规","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽640，椅高1200","张",2]
["办公区"]
[34,"六人位",{"$f":"_xlfn.DISPIMG(\"ID_DAAFFE4EFED349D6AA5F57E037830BF0\",1)","v":"=DISPIMG(\"ID_DAAFFE4EFED349D6AA5F57E037830BF0\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","3600*12008750","组",3]
[35,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_A78DA6497DBF4E6AABB47A7B0B92DBFE\",1)","v":"=DISPIMG(\"ID_A78DA6497DBF4E6AABB47A7B0B92DBFE\",1)"},null,"常规","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽490，椅高1060","张",18]
["异形办公区"]
[36,"8人位",{"$f":"_xlfn.DISPIMG(\"ID_DD9851AE919A4FFBBCA80937BA857658\",1)","v":"=DISPIMG(\"ID_DD9851AE919A4FFBBCA80937BA857658\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","5600*2500*750","组",1]
[37,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_729C64FD84CF4E3AB4D79D647DF32F4F\",1)","v":"=DISPIMG(\"ID_729C64FD84CF4E3AB4D79D647DF32F4F\",1)"},null,"白橘","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽640，椅高1200","张",8]
["水吧台"]
[38,"洽谈桌",{"$f":"_xlfn.DISPIMG(\"ID_A415429B155C4BAD91F54F09B6DF9332\",1)","v":"=DISPIMG(\"ID_A415429B155C4BAD91F54F09B6DF9332\",1)"},null,"一桌四椅","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","洽谈桌Φ800*750，洽谈椅：常规","套",4]
["四楼合计"]

{"sheet":"五楼","index":2,"n_rows":46,"n_cols":11,"rows_kept":46,"merged":[[0,0,0,10],[2,0,2,10],[6,0,6,10],[9,0,9,10],[16,0,16,10],[19,0,19,10],[25,0,25,10],[29,0,29,10],[32,0,32,10],[37,0,37,10],[41,0,41,10],[45,0,45,9]]}
["汇创谷（盐城）科技企业孵化器办公家具采购项目（5楼） 报价清单"]
["序号","项目名称","图片","名称","颜色","材质说明","规格","单位","数量","单价","总价"]
["公共办公室"]
[1,"6人位",{"$f":"_xlfn.DISPIMG(\"ID_114E664FB4C142A19A112B9DA3167766\",1)","v":"=DISPIMG(\"ID_114E664FB4C142A19A112B9DA3167766\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","3600*1200*750","组",4]
[2,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_9C54D94CD5484B5DAF00CD00FA083AAB\",1)","v":"=DISPIMG(\"ID_9C54D94CD5484B5DAF00CD00FA083AAB\",1)"},null,"常规","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽490，椅高1060","张",24]
[3,"低柜",{"$f":"_xlfn.DISPIMG(\"ID_FACBDAE82CF54FB5B5B6EAB63B590341\",1)","v":"=DISPIMG(\"ID_FACBDAE82CF54FB5B5B6EAB63B590341\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","3200*400*800","组",1]
["办公室"]
[4,"办公桌",{"$f":"_xlfn.DISPIMG(\"ID_68EB9A26D8DE4C1C8055F53645421736\",1)","v":"=DISPIMG(\"ID_68EB9A26D8DE4C1C8055F53645421736\",1)"},null,"卡其灰","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1800*780","张",2]
[5,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_0F0CE421B86E44468EB47983BCFF0951\",1)","v":"=DISPIMG(\"ID_0F0CE421B86E44468EB47983BCFF0951\",1)"},"办公桌","灰绿","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","坐宽480,椅高1250","张",2]
["办公室"]
[6,"办公桌",{"$f":"_xlfn.DISPIMG(\"ID_D548CE4F7CA3424B9C8E5FC37160CFCB\",1)","v":"=DISPIMG(\"ID_D548CE4F7CA3424B9C8E5FC37160CFCB\",1)"},null,"图片色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1600*800*750","张",1]
[7,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_355C3C56633443DAA7B61401F3C0E2A5\",1)","v":"=DISPIMG(\"ID_355C3C56633443DAA7B61401F3C0E2A5\",1)"},null,"图片色","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","坐宽480,椅高1250","张",1]
[8,"沙发",{"$f":"_xlfn.DISPIMG(\"ID_05D2B125AA094B7FBC61A0D0EC838A74\",1)","v":"=DISPIMG(\"ID_05D2B125AA094B7FBC61A0D0EC838A74\",1)"},null,"可定色","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","1800*800","张",1]
[9,"茶几",{"$f":"_xlfn.DISPIMG(\"ID_D0A6E3CCE85346E4BC6488801EED6E2E\",1)","v":"=DISPIMG(\"ID_D0A6E3CCE85346E4BC6488801EED6E2E\",1)"},null,"茶几","铝合金茶玻","1300*700*400","张",1]
[10,"6人位",{"$f":"_xlfn.DISPIMG(\"ID_5D0BA96FA51E4D21B273C7523C666B48\",1)","v":"=DISPIMG(\"ID_5D0BA96FA51E4D21B273C7523C666B48\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","3600*1200*750","张",2]
[11,"员工椅",{"$f":"_xlfn.DISPIMG(\"ID_439147BB8C1946D4BCA039576D02CDC8\",1)","v":"=DISPIMG(\"ID_439147BB8C1946D4BCA039576D02CDC8\",1)"},"牌桌椅子","灰色","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","常规","张",12]
["直播间"]
[12,"办公桌",{"$f":"_xlfn.DISPIMG(\"ID_06976BD8CD3C4204973063747DB36131\",1)","v":"=DISPIMG(\"ID_06976BD8CD3C4204973063747DB36131\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1400*700*750","张",26]
[13,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_814E9B6A16C6443C960BFC109455551A\",1)","v":"=DISPIMG(\"ID_814E9B6A16C6443C960BFC109455551A\",1)"},null,"可定色","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","坐宽480,椅高1250","张",26]
["办公室"]
[14,"办公桌",{"$f":"_xlfn.DISPIMG(\"ID_711615D8583947BC8DB9296C17C75AE9\",1)","v":"=DISPIMG(\"ID_711615D8583947BC8DB9296C17C75AE9\",1)"},null,"卡其灰","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1600*800*750","张",1]
[15,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_2A45FAAF187F4BFC8112FB50CE89653E\",1)","v":"=DISPIMG(\"ID_2A45FAAF187F4BFC8112FB50CE89653E\",1)"},null,"灰绿","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","坐宽480,椅高1250","张",1]
[16,"四人位",{"$f":"_xlfn.DISPIMG(\"ID_557B062FF15343F38AE2B019D5820B64\",1)","v":"=DISPIMG(\"ID_557B062FF15343F38AE2B019D5820B64\",1)"},null,null,"1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","2400*1200*750","组",1]
[17,"联排两人位",{"$f":"_xlfn.DISPIMG(\"ID_FCB6EDD4241A4E6FA2B8CAA040ADD989\",1)","v":"=DISPIMG(\"ID_FCB6EDD4241A4E6FA2B8CAA040ADD989\",1)"},null,"可定色是","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","2400*600*750","组",1]
[18,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_AE8C67FB5BAB487997A6E973B4A71CA5\",1)","v":"=DISPIMG(\"ID_AE8C67FB5BAB487997A6E973B4A71CA5\",1)"},null,"黑绿","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽490，椅高1060","张",6]
["办公区域95平"]
[19,"六人位",{"$f":"_xlfn.DISPIMG(\"ID_9855DB88CF194D7A817C7E76645E9E14\",1)","v":"=DISPIMG(\"ID_9855DB88CF194D7A817C7E76645E9E14\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","3600*1200*750","张",2]
[20,"八人位",{"$f":"_xlfn.DISPIMG(\"ID_17C1592614544FF0AB4F20C24CBABC50\",1)","v":"=DISPIMG(\"ID_17C1592614544FF0AB4F20C24CBABC50\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","4800*1200*750","张",2]
[21,"员工椅",{"$f":"_xlfn.DISPIMG(\"ID_7838467F92A340E1B921A56B3A82E66A\",1)","v":"=DISPIMG(\"ID_7838467F92A340E1B921A56B3A82E66A\",1)"},null,"常规","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽490，椅高1060","张",28]
["小会议室"]
[22,"会议桌",{"$f":"_xlfn.DISPIMG(\"ID_68E4D64BD379482784FF6327FA4B2CDF\",1)","v":"=DISPIMG(\"ID_68E4D64BD379482784FF6327FA4B2CDF\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","2000*1000*750","组",2]
[23,"会议椅",{"$f":"_xlfn.DISPIMG(\"ID_0C8C4C2FEF58420A872F1A5F90ADD938\",1)","v":"=DISPIMG(\"ID_0C8C4C2FEF58420A872F1A5F90ADD938\",1)"},null,"常规","1、面料:选优质PU,耐磨性强,阻燃,经防污处理,清洁方便；\n\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n\n钢脚管壁2.0","坐宽56，椅高95","张",6]
["办公室"]
[24,"办公桌",{"$f":"_xlfn.DISPIMG(\"ID_9271BA09EAE741059C6AF5A424E95140\",1)","v":"=DISPIMG(\"ID_9271BA09EAE741059C6AF5A424E95140\",1)"},null,"胡桃色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1600*800*750","组",1]
[25,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_227D946263E44AEE9207B9387A978FB3\",1)","v":"=DISPIMG(\"ID_227D946263E44AEE9207B9387A978FB3\",1)"},null,null,"\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","坐宽480,椅高1250","组",1]
[26,"沙发",{"$f":"_xlfn.DISPIMG(\"ID_57BFAEB1651644688D6576617941A664\",1)","v":"=DISPIMG(\"ID_57BFAEB1651644688D6576617941A664\",1)"},null,"可定色","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","1850*850*820","张",1]
[27,"茶几",{"$f":"_xlfn.DISPIMG(\"ID_EC09E0302DCA4B79ABCD54F544B33367\",1)","v":"=DISPIMG(\"ID_EC09E0302DCA4B79ABCD54F544B33367\",1)"},null,"图片色","铝合金茶玻","1300*700*400","张",1]
["办公区123平"]
[28,"十二人位",{"$f":"_xlfn.DISPIMG(\"ID_6907BA129F4347C8AAB4DD341795FF1F\",1)","v":"=DISPIMG(\"ID_6907BA129F4347C8AAB4DD341795FF1F\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","7200*1200*750","组",1]
[29,"六人位",{"$f":"_xlfn.DISPIMG(\"ID_49FF911B7CF942C3BA623226B38DBF05\",1)","v":"=DISPIMG(\"ID_49FF911B7CF942C3BA623226B38DBF05\",1)"},null,"白橘","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","3600*1200*750","组",1]
[30,"员工椅",{"$f":"_xlfn.DISPIMG(\"ID_92F430C32E1649F9BE7D43C5895526BA\",1)","v":"=DISPIMG(\"ID_92F430C32E1649F9BE7D43C5895526BA\",1)"},null,"可定色","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽490，椅高1060","组",18]
["办公室"]
[31,"办公桌",{"$f":"_xlfn.DISPIMG(\"ID_410E52F99254419F9713947283080024\",1)","v":"=DISPIMG(\"ID_410E52F99254419F9713947283080024\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1600*800*750","张",1]
[32,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_FD6205CEA89C4959AFEB18DEC02F22F8\",1)","v":"=DISPIMG(\"ID_FD6205CEA89C4959AFEB18DEC02F22F8\",1)"},null,"常规","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","坐宽480,椅高1250","张",1]
[33,"洽谈桌",{"$f":"_xlfn.DISPIMG(\"ID_D21BFAE983A74C0D827892ACED01F5CB\",1)","v":"=DISPIMG(\"ID_D21BFAE983A74C0D827892ACED01F5CB\",1)"},null,"一桌四椅","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","洽谈桌Φ800*750，洽谈椅：常规","张",1]
["五楼合计"]

{"sheet":"六楼","index":3,"n_rows":70,"n_cols":11,"rows_kept":70,"merged":[[0,0,0,10],[2,0,2,10],[8,0,8,10],[15,0,15,10],[20,0,20,10],[27,0,27,10],[30,0,30,10],[33,0,33,10],[38,0,38,10],[41,0,41,10],[44,0,44,10],[49,0,49,10],[54,0,54,10],[58,0,58,10],[61,0,61,10],[64,0,64,10],[69,0,69,9]]}
["汇创谷（盐城）科技企业孵化器办公家具采购项目（6楼） 报价清单"]
["序号","项目名称","图片","名称","颜色","材质说明","规格","单位","数量","单价","总价"]
["办公室（24平）"]
[1,"办公桌",{"$f":"_xlfn.DISPIMG(\"ID_E49873D00BEB421A815F0D252E9D2D32\",1)","v":"=DISPIMG(\"ID_E49873D00BEB421A815F0D252E9D2D32\",1)"},null,null,"1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1600*800*750","张",3]
[2,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_F62A932C61024430BCBF32D5F33B4BA1\",1)","v":"=DISPIMG(\"ID_F62A932C61024430BCBF32D5F33B4BA1\",1)"},null,null,"\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽490，椅高1060","张",3]
[3,"班前椅子",{"$f":"_xlfn.DISPIMG(\"ID_836A6CEF39FA451493A372CBE669AE9C\",1)","v":"=DISPIMG(\"ID_836A6CEF39FA451493A372CBE669AE9C\",1)"},null,null,"\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽490，椅高980","张",6]
[4,"三人位",{"$f":"_xlfn.DISPIMG(\"ID_D4D4D82B90784736A7B918F441B261A7\",1)","v":"=DISPIMG(\"ID_D4D4D82B90784736A7B918F441B261A7\",1)"},null,null,"采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","1800*780*850","组",1]
[5,"茶几",{"$f":"_xlfn.DISPIMG(\"ID_AD3407C08443438E9892377547AD6715\",1)","v":"=DISPIMG(\"ID_AD3407C08443438E9892377547AD6715\",1)"},"办公桌","1200*600","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1200*600*400","组",1]
["办公室（26平）"]
[6,"办公桌",{"$f":"_xlfn.DISPIMG(\"ID_06AB40CB77CF4913AED77967D25DFF7D\",1)","v":"=DISPIMG(\"ID_06AB40CB77CF4913AED77967D25DFF7D\",1)"},null,"图片色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1600*800*750","张",1]
[7,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_D43E6F871D96495993B10FCED894F292\",1)","v":"=DISPIMG(\"ID_D43E6F871D96495993B10FCED894F292\",1)"},null,"图片色","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽640，椅高1200","张",1]
[8,"沙发",{"$f":"_xlfn.DISPIMG(\"ID_589C055311994AE4AD3B73A7DF5BCCEC\",1)","v":"=DISPIMG(\"ID_589C055311994AE4AD3B73A7DF5BCCEC\",1)"},null,"可定色","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","1800*780*850","张",1]
[9,"茶几",{"$f":"_xlfn.DISPIMG(\"ID_E8603D854C3B47E2AE761E322F8F2AB5\",1)","v":"=DISPIMG(\"ID_E8603D854C3B47E2AE761E322F8F2AB5\",1)"},null,"白色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1200*600*400","张",1]
[10,"工作位",{"$f":"_xlfn.DISPIMG(\"ID_CF649FEC12724AFE8EC9D2AFA52061F6\",1)","v":"=DISPIMG(\"ID_CF649FEC12724AFE8EC9D2AFA52061F6\",1)"},null,null,"1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1200*1200*750","套",1]
[11,"椅子",{"$f":"_xlfn.DISPIMG(\"ID_6CAA45152EE146EEAEF39D90049DB485\",1)","v":"=DISPIMG(\"ID_6CAA45152EE146EEAEF39D90049DB485\",1)"},null,null,"\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽490，椅高1060","套",2]
["公共办公(136平)"]
[12,"6人位",{"$f":"_xlfn.DISPIMG(\"ID_20C93AD249B74F4BBF0CCD84AF3C50F6\",1)","v":"=DISPIMG(\"ID_20C93AD249B74F4BBF0CCD84AF3C50F6\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","3600*1200*750","张",2]
[13,"3人单排",{"$f":"_xlfn.DISPIMG(\"ID_3583B900814842B4AC8BEA23B50E7FB7\",1)","v":"=DISPIMG(\"ID_3583B900814842B4AC8BEA23B50E7FB7\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","3600*600*750","张",1]
[14,"员工椅",{"$f":"_xlfn.DISPIMG(\"ID_C8D696E38D9F4329B64A42F8202367C9\",1)","v":"=DISPIMG(\"ID_C8D696E38D9F4329B64A42F8202367C9\",1)"},"牌桌椅子","灰色","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽490，椅高1060","张",15]
[15,"低柜",{"$f":"_xlfn.DISPIMG(\"ID_248B739480264FFBB2096337D609D174\",1)","v":"=DISPIMG(\"ID_248B739480264FFBB2096337D609D174\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","3600*400*800","张",1]
["办公室"]
[16,"办公桌",{"$f":"_xlfn.DISPIMG(\"ID_8756BFC196BA4AA8B6942D73E39B6B83\",1)","v":"=DISPIMG(\"ID_8756BFC196BA4AA8B6942D73E39B6B83\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1600*800*750","张",1]
[17,"椅子",{"$f":"_xlfn.DISPIMG(\"ID_5EA95B4A405D465C89EE552C4F2D4F84\",1)","v":"=DISPIMG(\"ID_5EA95B4A405D465C89EE552C4F2D4F84\",1)"},null,null,"\"1、面料:选进口牛皮,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽640，椅高1200","张",1]
[18,"班前椅子",{"$f":"_xlfn.DISPIMG(\"ID_278C588E6AC946CF83A265F933FCA8CA\",1)","v":"=DISPIMG(\"ID_278C588E6AC946CF83A265F933FCA8CA\",1)"},null,null,"\"1、面料:选进口西皮,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","常规","张",2]
[19,"沙发",{"$f":"_xlfn.DISPIMG(\"ID_1ADA605698354105B7EEDA95677231D6\",1)","v":"=DISPIMG(\"ID_1ADA605698354105B7EEDA95677231D6\",1)"},null,null,"采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","1800*780*850","张",1]
[20,"茶几",{"$f":"_xlfn.DISPIMG(\"ID_C80F2C66270C4CA39AC9561F64D17C48\",1)","v":"=DISPIMG(\"ID_C80F2C66270C4CA39AC9561F64D17C48\",1)"},null,null,"1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1200*600*400","张",1]
[21,"茶台（1桌+5椅）",{"$f":"_xlfn.DISPIMG(\"ID_F7DEB980D4C74738B99B759AFD61F5A9\",1)","v":"=DISPIMG(\"ID_F7DEB980D4C74738B99B759AFD61F5A9\",1)"},null,null,"1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1600*750*750","套",1]
["办公室"]
[22,"办公桌",{"$f":"_xlfn.DISPIMG(\"ID_88210A1C06A34E8B9668AD0DF4578F3C\",1)","v":"=DISPIMG(\"ID_88210A1C06A34E8B9668AD0DF4578F3C\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1600*800*750","张",2]
[23,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_81338E76425B489399CC6B42793822BA\",1)","v":"=DISPIMG(\"ID_81338E76425B489399CC6B42793822BA\",1)"},null,null,"\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽640，椅高1200","张",2]
["公共办公(76平)"]
[24,"六人位",{"$f":"_xlfn.DISPIMG(\"ID_B99827A6F2CA4775985EBC7554B94DDE\",1)","v":"=DISPIMG(\"ID_B99827A6F2CA4775985EBC7554B94DDE\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","3600*1200*750","组",2]
[25,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_AF1F2D5D31544DE6B752CE7558DE5977\",1)","v":"=DISPIMG(\"ID_AF1F2D5D31544DE6B752CE7558DE5977\",1)"},null,null,"\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽490，椅高1060","张",12]
["办公室"]
[26,"办公桌",{"$f":"_xlfn.DISPIMG(\"ID_9A414DC3428C47559F92ABF67AFEEEFB\",1)","v":"=DISPIMG(\"ID_9A414DC3428C47559F92ABF67AFEEEFB\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1600*800*750","组",1]
[27,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_846F17ED7C7746389C697EC49B9B452F\",1)","v":"=DISPIMG(\"ID_846F17ED7C7746389C697EC49B9B452F\",1)"},null,"白橘","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽640，椅高1200","组",1]
[28,"沙发",{"$f":"_xlfn.DISPIMG(\"ID_3209C86CDFF54B8EAD08D61D05132EF2\",1)","v":"=DISPIMG(\"ID_3209C86CDFF54B8EAD08D61D05132EF2\",1)"},null,"可定色","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","1800*780*850","组",1]
[29,"茶几",{"$f":"_xlfn.DISPIMG(\"ID_A37184168154478E88A0001F57782758\",1)","v":"=DISPIMG(\"ID_A37184168154478E88A0001F57782758\",1)"},null,"白色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1200*600*400","张",1]
["办公室（151平）"]
[30,"十人人位",{"$f":"_xlfn.DISPIMG(\"ID_C47CAF355D4441B981796F3D1436E0B4\",1)","v":"=DISPIMG(\"ID_C47CAF355D4441B981796F3D1436E0B4\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","6000*1200*750 ","组",2]
[31,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_2F3C4C0D6CDC4236ACA03D515A01F215\",1)","v":"=DISPIMG(\"ID_2F3C4C0D6CDC4236ACA03D515A01F215\",1)"},null,null,"\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽490，椅高1060","张",20]
["休闲区"]
[32,"休闲沙发",{"$f":"_xlfn.DISPIMG(\"ID_E6B20CB043544999806D4884309CBAC5\",1)","v":"=DISPIMG(\"ID_E6B20CB043544999806D4884309CBAC5\",1)"},null,"胡桃色","采用优质布面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","2000*600*850","组",1]
[33,"茶几",{"$f":"_xlfn.DISPIMG(\"ID_A651BA949ABE42C6A89D96AC4C77E7BE\",1)","v":"=DISPIMG(\"ID_A651BA949ABE42C6A89D96AC4C77E7BE\",1)"},null,"灰白","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1200*600*400","组",1]
["办公区"]
[34,"办公桌",{"$f":"_xlfn.DISPIMG(\"ID_5C5AC9BBE7694B6DBB716FAD0FC39B94\",1)","v":"=DISPIMG(\"ID_5C5AC9BBE7694B6DBB716FAD0FC39B94\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1600*800*750","组",1]
[35,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_B428170821574463AEEE8836BD2803CC\",1)","v":"=DISPIMG(\"ID_B428170821574463AEEE8836BD2803CC\",1)"},null,"白橘","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽640，椅高1200","组",1]
[36,"沙发",{"$f":"_xlfn.DISPIMG(\"ID_0FCD3CD190A740A99DC976E2FA7226C1\",1)","v":"=DISPIMG(\"ID_0FCD3CD190A740A99DC976E2FA7226C1\",1)"},null,"可定色","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","1800*780*850","组",1]
[37,"茶几",{"$f":"_xlfn.DISPIMG(\"ID_5B927E84D76F4815A0C5BA54532F6736\",1)","v":"=DISPIMG(\"ID_5B927E84D76F4815A0C5BA54532F6736\",1)"},null,"白色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1200*600*400","张",1]
["办公室"]
[38,"办公桌",{"$f":"_xlfn.DISPIMG(\"ID_C74A4869FF9444EBB1A148E4F6B19468\",1)","v":"=DISPIMG(\"ID_C74A4869FF9444EBB1A148E4F6B19468\",1)"},null,"灰","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1600*800*750","张",1]
[39,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_87F519A811314E69B73B51ED3E6E1108\",1)","v":"=DISPIMG(\"ID_87F519A811314E69B73B51ED3E6E1108\",1)"},null,"白橘","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽640，椅高1200","张",1]
[40,"沙发",{"$f":"_xlfn.DISPIMG(\"ID_6BC26679C6B74714BF54BE17C8476512\",1)","v":"=DISPIMG(\"ID_6BC26679C6B74714BF54BE17C8476512\",1)"},null,"可定色","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","1800*780*850","张",1]
[41,"茶几",{"$f":"_xlfn.DISPIMG(\"ID_CCBC1AED292243B7AB9D6DDCC863411D\",1)","v":"=DISPIMG(\"ID_CCBC1AED292243B7AB9D6DDCC863411D\",1)"},null,"白","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1200*600*400","张",1]
["办公区139平"]
[42,"六人位",{"$f":"_xlfn.DISPIMG(\"ID_AC90702FE37340E988FBB050B3E9955E\",1)","v":"=DISPIMG(\"ID_AC90702FE37340E988FBB050B3E9955E\",1)"},null,null,"1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","3600*1200*750","组",3]
[43,"员工椅",{"$f":"_xlfn.DISPIMG(\"ID_647EFCAF960941B7A6961E4691092E73\",1)","v":"=DISPIMG(\"ID_647EFCAF960941B7A6961E4691092E73\",1)"},null,"常规","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽490，椅高1060","张",18]
[44,"低柜",{"$f":"_xlfn.DISPIMG(\"ID_1185695CE8F1422D86639472C1B214C4\",1)","v":"=DISPIMG(\"ID_1185695CE8F1422D86639472C1B214C4\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","3600*400*800","张",1]
["办公室"]
[45,"办公桌",{"$f":"_xlfn.DISPIMG(\"ID_D211426A078F4F2D982D0CA5A49A6977\",1)","v":"=DISPIMG(\"ID_D211426A078F4F2D982D0CA5A49A6977\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1600*800*750","张",2]
[46,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_6248A8FD9246401EB3AB1920A5759515\",1)","v":"=DISPIMG(\"ID_6248A8FD9246401EB3AB1920A5759515\",1)"},null,"常规","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽640，椅高1200","张",2]
["办公区139平，77平，80平"]
[47,"六人位",{"$f":"_xlfn.DISPIMG(\"ID_F31CFE39C87642279BF0AAFCB6C1CFC2\",1)","v":"=DISPIMG(\"ID_F31CFE39C87642279BF0AAFCB6C1CFC2\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","3600*1200*750","组",7]
[48,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_E1EC7B95648C4D7BB900DF15654D45B3\",1)","v":"=DISPIMG(\"ID_E1EC7B95648C4D7BB900DF15654D45B3\",1)"},null,"常规","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽490，椅高1060","张",42]
["异形办公区"]
[49,"办公桌",{"$f":"_xlfn.DISPIMG(\"ID_2754E33A303947C7A2C8E07A3EA1CEA1\",1)","v":"=DISPIMG(\"ID_2754E33A303947C7A2C8E07A3EA1CEA1\",1)"},null,"可定色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1600*800*750","组",1]
[50,"办公椅",{"$f":"_xlfn.DISPIMG(\"ID_449D0773E2D1474FA0B3725198121059\",1)","v":"=DISPIMG(\"ID_449D0773E2D1474FA0B3725198121059\",1)"},null,"白橘","\"1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用 发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；\n钢脚管壁2.0\"","椅宽640，椅高1200","组",1]
[51,"沙发",{"$f":"_xlfn.DISPIMG(\"ID_CDE63ABFA90845AAA8F52015644410D9\",1)","v":"=DISPIMG(\"ID_CDE63ABFA90845AAA8F52015644410D9\",1)"},null,"可定色","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","1800*780*850","组",1]
[52,"茶几",{"$f":"_xlfn.DISPIMG(\"ID_96875D3BBB2F41CDB1C81DDAC6D4D60D\",1)","v":"=DISPIMG(\"ID_96875D3BBB2F41CDB1C81DDAC6D4D60D\",1)"},null,"白色","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5、具有防水、防烫、防污、防酸、防碱、防火。 ","1200*600*400","张",1]
["六楼合计"]