{"text_format":"3","workbook":"xlsx","n_sheets":4,"sheets":["汇总表","十二楼","十三楼","十四楼"],"not_rendered":{"images":19,"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"汇总表","index":0,"n_rows":6,"n_cols":3,"rows_kept":6,"merged":[[0,0,0,2],[5,0,5,1]]}
["未来科技城A1（12-14）层矩阵孵化器办公家具采购项目  报价汇总表"]
["序号","楼层","总计价格（含税）"]
[1,"十二楼"]
[2,"十三楼"]
[3,"十四楼"]
["合计"]

{"sheet":"十二楼","index":1,"n_rows":63,"n_cols":10,"rows_kept":63,"merged":[[0,0,0,9],[2,0,2,9],[9,0,9,9],[17,0,17,9],[25,0,25,9],[34,1,34,9],[42,0,42,9],[50,1,50,7],[56,0,56,9],[62,0,62,8]]}
["未来科技城A1（12-14）层矩阵孵化器办公家具采购项目 十二楼"]
["序号","项目名称","图片","颜色","规格","材质说明","单位","数量","固定全费用综合单价（元）","合计（元）"]
["办公室（67平）"]
[1,"前台",null,"图片色","2200*700*1100","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[2,"4人工位",{"$f":"_xlfn.DISPIMG(\"ID_6331329FEA0742F89D0B605368340EE4\",1)","v":"=DISPIMG(\"ID_6331329FEA0742F89D0B605368340EE4\",1)"},"图片色","2400*1200*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",2]
[3,"单人工位",null,"图片色","1600*800*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",2]
[4,"洽谈桌椅",null,"图片色","1桌4椅（灰色白色岩板）\n直径80CM","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[5,"办公椅",null,"黑色","1100*600","1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用杜邦公司的PU成型发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；钢脚管壁2.0","张",13]
[6,"老板椅",null,"图片色","1280*700","1、面料：选用意大利优质进口头层牛皮；                                          2、海绵：优质沐森高回弹海绵，椅座50#高密度海绵，椅背40#高密度海绵；                                                                                               3、曲木板：密度≥600kg/m3，含水率≤9%，经高温蒸煮、高温干燥、高温层压。不变形、不虫蛀、不霉；                                                                                                                                               4、底盘及气杆：采用意大利进口底盘， 气压升降棒，气动升降，倾仰调节；                                                                     5、椅脚及椅轮：黑色强化PU防震静音轮；","张",2]
["办公室（76平）"]
[7,"前台",null,"图片色","2200*700*1100","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[8,"4人工位",null,"图片色","2400*1200*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",2]
[9,"单人工位",null,"图片色","1600*800*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",2]
[10,"双人沙发",null,"图片色","1700*775","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","张",2]
[11,"茶几",null,"图片色","1000*500","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",2]
[12,"办公椅",null,"黑色","1100*600","1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用杜邦公司的PU成型发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；钢脚管壁2.0","张",13]
[13,"老板椅",null,"图片色","1280*700","1、面料：选用意大利优质进口头层牛皮；                                          2、海绵：优质沐森高回弹海绵，椅座50#高密度海绵，椅背40#高密度海绵；                                                                                               3、曲木板：密度≥600kg/m3，含水率≤9%，经高温蒸煮、高温干燥、高温层压。不变形、不虫蛀、不霉；                                                                                                                                               4、底盘及气杆：采用意大利进口底盘， 气压升降棒，气动升降，倾仰调节；                                                                     5、椅脚及椅轮：黑色强化PU防震静音轮；","张",2]
["办公室（71平）"]
[14,"前台",null,"图片色","2200*700*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[15,"洽谈沙发",null,"图片色","1500*840*860","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","张",2]
[16,"茶几",null,"图片色","1000*500","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",2]
[17,"4人工位",null,"图片色","2400*1200*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",2]
[18,"单人工位",null,"图片色","1600*800*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",2]
[19,"办公椅",null,"黑色","1100*600","1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用杜邦公司的PU成型发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；钢脚管壁2.0","张",13]
[20,"老板椅",null,"图片色","1280*700","1、面料：选用意大利优质进口头层牛皮；                                          2、海绵：优质沐森高回弹海绵，椅座50#高密度海绵，椅背40#高密度海绵；                                                                                               3、曲木板：密度≥600kg/m3，含水率≤9%，经高温蒸煮、高温干燥、高温层压。不变形、不虫蛀、不霉；                                                                                                                                               4、底盘及气杆：采用意大利进口底盘， 气压升降棒，气动升降，倾仰调节；                                                                     5、椅脚及椅轮：黑色强化PU防震静音轮；","张",2]
["办公室（137平）"]
[21,"前台",null,"图片色","2200*700*1100","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[22,"4人工位",null,"图片色","2400*1200*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",3]
[23,"6人工位",null,"图片色","4200*1400*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[24,"单人工位",null,"图片色","1600*800*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",2]
[25,"沙发",null,"图片色","1700*775","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","张",2]
[26,"茶几",null,"图片色","1000*500","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",2]
[27,"办公椅",null,"黑色","1100*600","1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用杜邦公司的PU成型发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；钢脚管壁2.0","张",23]
[28,"老板椅",null,"图片色","1280*700","1、面料：选用意大利优质进口头层牛皮；                                          2、海绵：优质沐森高回弹海绵，椅座50#高密度海绵，椅背40#高密度海绵；                                                                                               3、曲木板：密度≥600kg/m3，含水率≤9%，经高温蒸煮、高温干燥、高温层压。不变形、不虫蛀、不霉；                                                                                                                                               4、底盘及气杆：采用意大利进口底盘， 气压升降棒，气动升降，倾仰调节；                                                                     5、椅脚及椅轮：黑色强化PU防震静音轮；","张",2]
[null,"办公室（95平）"]
[29,"前台",null,"图片色","2600*700*1100","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[30,"4人工位",null,"图片色","2400*1200*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[31,"6人工位",null,"图片色","4200*1400*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[32,"单人工位",null,"图片色","1600*800*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",2]
[33,"老板椅",null,"图片色","1280*700","1、面料：选用意大利优质进口头层牛皮；                                          2、海绵：优质沐森高回弹海绵，椅座50#高密度海绵，椅背40#高密度海绵；                                                                                               3、曲木板：密度≥600kg/m3，含水率≤9%，经高温蒸煮、高温干燥、高温层压。不变形、不虫蛀、不霉；                                                                                                                                               4、底盘及气杆：采用意大利进口底盘， 气压升降棒，气动升降，倾仰调节；                                                                     5、椅脚及椅轮：黑色强化PU防震静音轮；","张",2]
[34,"会议桌",null,"图片色","2000*1000*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[35,"办公椅",null,"黑色","1100*600","1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用杜邦公司的PU成型发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；钢脚管壁2.0","张",23]
["办公室（107平）"]
[36,"前台",null,"图片色","2200*700*1100","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[37,"4人工位",null,"图片色","2400*1200*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[38,"6人工位",null,"图片色","4200*1400*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[39,"单人工位",null,"图片色","1600*800*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",2]
[40,"老板椅",null,"图片色","1280*700","1、面料：选用意大利优质进口头层牛皮；                                          2、海绵：优质沐森高回弹海绵，椅座50#高密度海绵，椅背40#高密度海绵；                                                                                               3、曲木板：密度≥600kg/m3，含水率≤9%，经高温蒸煮、高温干燥、高温层压。不变形、不虫蛀、不霉；                                                                                                                                               4、底盘及气杆：采用意大利进口底盘， 气压升降棒，气动升降，倾仰调节；                                                                     5、椅脚及椅轮：黑色强化PU防震静音轮；","张",2]
[41,"会议桌",null,"图片色","3000*1200*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[42,"办公椅",null,"黑色","1100*600","1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用杜邦公司的PU成型发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；钢脚管壁2.0","张",25]
[null,"办公室（92平）"]
[43,"前台",null,"图片色","1900*700*1100","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[44,"6人工位",null,"图片色","4200*1400*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[45,"单人工位",null,"图片色","1600*800*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[46,"沙发",null,"图片色","1700*775","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","张",1]
[47,"茶几",null,"图片色","1000*500","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",1]
["办公室（73平）"]
[48,"前台",null,"图片色","1900*700*1100","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[49,"6人工位",null,"图片色","4200*1400*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[50,"单人工位",null,"图片色","1600*800*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[51,"沙发",null,"图片色","1700*775","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","张",1]
[52,"茶几",null,"图片色","1000*500","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂： 进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",1]
["十二楼合计"]

{"sheet":"十三楼","index":2,"n_rows":57,"n_cols":10,"rows_kept":57,"merged":[[0,0,0,9],[2,0,2,9],[9,0,9,9],[17,0,17,9],[25,0,25,9],[34,0,34,9],[42,0,42,9],[50,0,50,9],[56,0,56,8]]}
["未来科技城A1（12-14）层矩阵孵化器办公家具采购项目 十三楼"]
["序号","项目名称","图片","颜色","规格","材质说明","单位","数量","固定全费用综合单价（元）","合计（元）"]
["办公室（67平）"]
[1,"前台",null,"图片色","2200*700*1100","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[2,"4人工位",null,"图片色","2400*1200*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",2]
[3,"单人工位",null,"图片色","1600*800*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",2]
[4,"洽谈桌椅",null,"图片色","1桌4椅（灰色白色岩板）\n直径80CM","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[5,"老板椅",null,"图片色","1280*700","1、面料：选用意大利优质进口头层牛皮；                                          2、海绵：优质沐森高回弹海绵，椅座50#高密度海绵，椅背40#高密度海绵；                                                                                               3、曲木板：密度≥600kg/m3，含水率≤9%，经高温蒸煮、高温干燥、高温层压。不变形、不虫蛀、不霉；                                                                                                                                               4、底盘及气杆：采用意大利进口底盘， 气压升降棒，气动升降，倾仰调节；                                                                     5、椅脚及椅轮：黑色强化PU防震静音轮；","张",2]
[6,"办公椅",null,"黑色","1100*600","1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用杜邦公司的PU成型发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；钢脚管壁2.0","张",13]
["办公室（67平）"]
[7,"前台",null,"图片色","2200*700*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[8,"4人工位",null,"图片色","2400*1200*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",2]
[9,"单人工位",null,"图片色","1600*800*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",2]
[10,"双人沙发",null,"图片色","1700*775","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","张",2]
[11,"茶几",null,"图片色","1000*500","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",2]
[12,"办公椅",null,"黑色","1100*600","1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用杜邦公司的PU成型发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；钢脚管壁2.0","张",13]
[13,"老板椅",null,"图片色","1280*700","1、面料：选用意大利优质进口头层牛皮；                                          2、海绵：优质沐森高回弹海绵，椅座50#高密度海绵，椅背40#高密度海绵；                                                                                               3、曲木板：密度≥600kg/m3，含水率≤9%，经高温蒸煮、高温干燥、高温层压。不变形、不虫蛀、不霉；                                                                                                                                               4、底盘及气杆：采用意大利进口底盘， 气压升降棒，气动升降，倾仰调节；                                                                     5、椅脚及椅轮：黑色强化PU防震静音轮；","张",2]
["办公室（71平）"]
[14,"前台",null,"图片色","2200*700*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[15,"双人沙发",null,"图片色","1700*775","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","张",1]
[16,"茶几",null,"图片色","1000*500","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[17,"4人工位",null,"图片色","2400*1200*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",2]
[18,"单人工位",null,"图片色","1600*800*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",2]
[19,"老板椅",null,"图片色","1280*700","1、面料：选用意大利优质进口头层牛皮；                                          2、海绵：优质沐森高回弹海绵，椅座50#高密度海绵，椅背40#高密度海绵；                                                                                               3、曲木板：密度≥600kg/m3，含水率≤9%，经高温蒸煮、高温干燥、高温层压。不变形、不虫蛀、不霉；                                                                                                                                               4、底盘及气杆：采用意大利进口底盘， 气压升降棒，气动升降，倾仰调节；                                                                     5、椅脚及椅轮：黑色强化PU防震静音轮；","张",2]
[20,"办公椅",null,"黑色","1100*600","1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用杜邦公司的PU成型发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；钢脚管壁2.0","张",13]
["办公室（137平）"]
[21,"前台",null,"图片色","2400*700*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[22,"4人工位",null,"图片色","2400*1200*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",3]
[23,"6人工位",null,"图片色","4200*1400*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[24,"单人工位",null,"图片色","1600*800*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",2]
[25,"双人沙发",null,"图片色","1700*775","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","张",2]
[26,"茶几",null,"图片色","1000*500","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",2]
[27,"老板椅",null,"图片色","1280*700","1、面料：选用意大利优质进口头层牛皮；                                          2、海绵：优质沐森高回弹海绵，椅座50#高密度海绵，椅背40#高密度海绵；                                                                                               3、曲木板：密度≥600kg/m3，含水率≤9%，经高温蒸煮、高温干燥、高温层压。不变形、不虫蛀、不霉；                                                                                                                                               4、底盘及气杆：采用意大利进口底盘， 气压升降棒，气动升降，倾仰调节；                                                                     5、椅脚及椅轮：黑色强化PU防震静音轮；","张",2]
[28,"办公椅",null,"黑色","1100*600","1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用杜邦公司的PU成型发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；钢脚管壁2.0","张",23]
["办公室（119平）"]
[29,"前台",null,"图片色","2600*700*1100","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[30,"4人工位",null,"图片色","2400*1200*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[31,"6人工位",null,"图片色","4200*1400*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[32,"单人工位",null,"图片色","1600*800*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",2]
[33,"会议桌",null,"会议桌","2000*1000*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[34,"老板椅",null,"图片色","1280*700","1、面料：选用意大利优质进口头层牛皮；                                          2、海绵：优质沐森高回弹海绵，椅座50#高密度海绵，椅背40#高密度海绵；                                                                                               3、曲木板：密度≥600kg/m3，含水率≤9%，经高温蒸煮、高温干燥、高温层压。不变形、不虫蛀、不霉；                                                                                                                                               4、底盘及气杆：采用意大利进口底盘， 气压升降棒，气动升降，倾仰调节；                                                                     5、椅脚及椅轮：黑色强化PU防震静音轮；","张",2]
[35,"办公椅",null,"黑色","1100*600","1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用杜邦公司的PU成型发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；钢脚管壁2.0","张",23]
["办公室（107平）"]
[36,"前台",null,"图片色","2200*700*1100","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[37,"4人工位",null,"图片色","2400*1200*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[38,"6人工位",null,"图片色","4200*1400*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[39,"单人工位",null,"图片色","1600*800*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",2]
[40,"会议桌",null,"图片色","3000*1200*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[41,"老板椅",null,"图片色","1280*700","1、面料：选用意大利优质进口头层牛皮；                                          2、海绵：优质沐森高回弹海绵，椅座50#高密度海绵，椅背40#高密度海绵；                                                                                               3、曲木板：密度≥600kg/m3，含水率≤9%，经高温蒸煮、高温干燥、高温层压。不变形、不虫蛀、不霉；                                                                                                                                               4、底盘及气杆：采用意大利进口底盘， 气压升降棒，气动升降，倾仰调节；                                                                     5、椅脚及椅轮：黑色强化PU防震静音轮；","张",2]
[42,"办公椅",null,"黑色","1100*600","1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用杜邦公司的PU成型发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；钢脚管壁2.0","张",25]
["办公室（181平）"]
[43,"前台",null,"图片色","2200*700*1100","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[44,"4人工位",null,"图片色","2400*1200*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",4]
[45,"单人工位",null,"图片色","1600*800*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","套",2]
[46,"双人沙发",null,"图片色","1700*775","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","张",2]
[47,"茶几",null,"图片色","1000*500","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张 度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；       \n5. 具有防水、防烫、防污、防酸、防碱、防火。","张",2]
["十三楼合计"]

{"sheet":"十四楼","index":3,"n_rows":62,"n_cols":10,"rows_kept":62,"merged":[[0,0,0,9],[2,0,2,9],[12,0,12,9],[18,0,18,9],[25,0,25,9],[34,1,34,7],[42,0,42,9],[49,1,49,7],[61,0,61,8]]}
["未来科技城A1（12-14）层矩阵孵化器办公家具采购项目 十四楼"]
["序号","项目名称","图片","颜色","规格","材质说明","单位","数量","固定全费用综合单价（元）","合计（元）"]
["办公室（96平）"]
[1,"前台",null,"图片色","2200*700*1100","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[2,"4人工位",null,"图片色","2400*1200*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[3,"6人工位",null,"图片色","3600*1200*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[4,"单人工位",null,"图片色","1600*800","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[5,"双人沙发",null,"图片色","1700*775","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","张",1]
[6,"茶几",null,"图片色","1000*500","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[7,"会议桌",null,"会议桌","2000*1000*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[8,"老板椅",null,"图片色","1280*700","1、面料：选用意大利优质进口头层牛皮；2、海绵：优质沐森高回弹海绵，椅座50#高密度海绵，椅背40#高密度海绵；3、曲木板：密度≥600kg/m3，含水率≤9%，经高温蒸煮、高温干燥、高温层压。不变形、不虫蛀、不霉；4、底盘及气杆：采用意大利进口底盘，气压升降棒，气动升降，倾仰调节；5、椅脚及椅轮：黑色强化PU防震静音轮；","张",2]
[9,"办公椅",null,"黑色","1100*600","1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用杜邦公司的PU成型发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；钢脚管壁2.0","张",23]
["办公室（90平）"]
[10,"前台",null,"图片色","4000*700*1100","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[11,"洽谈桌椅",null,"图片色","1桌4椅（灰色白色岩板）\n直径80CM","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","套",3]
[12,"3人位",null,"图片色","2270*900*880","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","张",1]
[13,"单人位",null,"图片色","1260*900*880","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","张",1]
[14,"茶几",null,"图片色","1200*650*430","岩板台面，金属脚架","张",1]
["办公室（51平）"]
[15,"前台",null,"图片色","2500*700*1100","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[16,"4人工位",null,"图片色","2400*1200*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[17,"2人工位",null,"图片色","1200*1200*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n6.具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[18,"单人工位",null,"图片色","1600*800","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[19,"老板椅",null,"图片色","1280*700","1、面料：选用意大利优质进口头层牛皮；2、海绵：优质沐森高回弹海绵，椅座50#高密度海绵，椅背40#高密度海绵；3、曲木板：密度≥600kg/m3，含水率≤9%，经高温蒸煮、高温干燥、高温层压。不变形、不虫蛀、不霉；4、底盘及气杆：采用意大利进口底盘，气压升降棒，气动升降，倾仰调节；5、椅脚及椅轮：黑色强化PU防震静音轮；","张",1]
[20,"办公椅",null,"黑色","1100*600","1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用杜邦公司的PU成型发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；钢脚管壁2.0","张",9]
["办公室（137平）"]
[21,"前台",null,"图片色","2600*700*1100","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[22,"4人工位",null,"图片色","2400*1200*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","套",4]
[23,"单人工位",null,"图片色","1600*800*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[24,"双人沙发",null,"图片色","1700*775","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","张",1]
[25,"茶几",null,"图片色","1000*500","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[26,"洽谈桌椅",null,"图片色","1桌4椅（灰色白色岩板）\n直径80CM","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[27,"老板椅",null,"图片色","1280*700","1、面料：选用意大利优质进口头层牛皮；2、海绵：优质沐森高回弹海绵，椅座50#高密度海绵，椅背40#高密度海绵；3、曲木板：密度≥600kg/m3，含水率≤9%，经高温蒸煮、高温干燥、高温层压。不变形、不虫蛀、不霉；4、底盘及气杆：采用意大利进口底盘，气压升降棒，气动升降，倾仰调节；5、椅脚及椅轮：黑色强化PU防震静音轮；","张",1]
[28,"办公椅",null,"黑色","1100*600","1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用杜邦公司的PU成型发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；钢脚管壁2.0","张",15]
[null,"办公室（119平）"]
[29,"前台",null,"图片色","2600*700*1100","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[30,"4人工位",null,"图片色","2400*1400*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[31,"6人工位",null,"图片色","4200*1400*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[32,"单人工位",null,"图片色","1600*800*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","套",2]
[33,"会议桌",null,"图片色","2000*1000*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[34,"老板椅",null,"图片色","1280*700","1、面料：选用意大利优质进口头层牛皮；2、海绵：优质沐森高回弹海绵，椅座50#高密度海绵，椅背40#高密度海绵；3、曲木板：密度≥600kg/m3，含水率≤9%，经高温蒸煮、高温干燥、高温层压。不变形、不虫蛀、不霉；4、底盘及气杆：采用意大利进口底盘，气压升降棒，气动升降，倾仰调节；5、椅脚及椅轮：黑色强化PU防震静音轮；","张",2]
[35,"办公椅",null,"黑色","1100*600","1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用杜邦公司的PU成型发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；钢脚管壁2.0","张",23]
["办公室（80平）"]
[36,"前台",null,"图片色","2600*700*1100","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[37,"单人工位",null,"图片色","1400*700*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[38,"单人工位",null,"图片色","1600*800*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","套",2]
[39,"6人工位",null,"图片色","4200*1400*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","套",1]
[40,"老板椅",null,"图片色","1280*700","1、面料：选用意大利优质进口头层牛皮；2、海绵：优质沐森高回弹海绵，椅座50#高密度海绵，椅背40#高密度海绵；3、曲木板：密度≥600kg/m3，含水率≤9%，经高温蒸煮、高温干燥、高温层压。不变形、不虫蛀、不霉；4、底盘及气杆：采用意大利进口底盘，气压升降棒，气动升降，倾仰调节；5、椅脚及椅轮：黑色强化PU防震静音轮；","张",2]
[41,"办公椅",null,"黑色","1100*600","1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用杜邦公司的PU成型发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；钢脚管壁2.0","张",12]
[null,"办公室（160平）"]
[42,"前台",null,"图片色","1800*700*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[43,"单人工位",null,"图片色","1800*800*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","套",3]
[44,"4人工位",null,"图片色","2400*1400*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","套",2]
[45,"会议桌",null,"图片色","3000*1200*750","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","张",1]
[46,"文件柜",null,"图片色","1800*850*390","基材：采用宝钢优质冷轧钢板厚度0.8mm。表面经酸洗磷化、恒温静电喷涂等13道工艺处理，产品喷涂塑粉附着力更强、不脱落、不生锈。进口绿色环保阿克苏塑粉，无毒、无副作用、无异味。品牌锁具，薄边设计，更引领潮流时尚。","个",2]
[47,"茶水柜",null,"图片色","1200*360*1000","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","个",1]
[48,"3人沙发",null,"图片色","1800*780","采用优质PU皮面料，透气性强，皮质柔软铁手，光滑耐磨，内框架采用依据人体学原理制造的多层板热压成型，经防虫、防腐处理，一次成型高密度泡棉。钢制下架.","张",5]
[49,"茶几",null,"图片色","1000*500","1、贴面板材：采用符合国家标准E1级环保三聚氰胺防火板，\n2、基材：进口中纤板,优质绿色环保产品,甲醛含量≤1.0mg/L密度≥760kg/m3,静曲张度≥51.2Mpa,吸水膨胀率≤8.1%.\n3、粘合剂：进口乳胶；\n4、封边用材：2mm厚PVC胶边，进口热熔胶；\n5.具有防水、防烫、防污、防酸、防碱、防火。","张",5]
[50,"老板椅",null,"图片色","1280*700","1、面料：选用意大利优质进口头层牛皮；2、海绵：优质沐森高回弹海绵，椅座50#高密度海绵，椅背40#高密度海绵；3、曲木板：密度≥600kg/m3，含水率≤9%，经高温蒸煮、高温干燥、高温层压。不变形、不虫蛀、不霉；4、底盘及气杆：采用意大利进口底盘，气压升降棒，气动升降，倾仰调节；5、椅脚及椅轮：黑色强化PU防震静音轮；","张",6]
[51,"办公椅",null,"黑色","1100*600","1、面料:选进口网布,耐磨性强,阻燃,经防污处理,清洁方便；\n2、辅料:采用杜邦公司的PU成型发泡高密度海绵,表面有一层保护面,可防氧化,防碎,经过HD测试永不变形；钢脚管壁2.0","张",34]
[52,"接待室",null,"原木色","常规","莲花桌（1.8米）+1梳背椅+4梳背客椅+博古架（含茶水柜、花架）","套",1]
["十四楼合计"]